#

##

##

    礦ision Build Log
    Project:
    F:\佳显电子\新程序\电子纸驱动程序更新20191008\AY\6.0\GDE060F3程序示例20190111\project\TCON_NEW.uvproj
    Project File Date:  10/09/2017

    Output:
    Build target 'Target 1'
    compiling main.c...
    linking...
    Program Size: Code=13996 RO-data=234256 RW-data=24 ZI-data=1632
    FromELF: creating hex file...
    ".\TCON_NEW.axf" - 0 Error(s), 0 Warning(s).
    Load "F:\\佳显电子\\新程序\\电子纸驱动程序更新20191008\\AY\\6.0\\GDE060F3程序示例20190111\\project\\TCON_NEW.axf"
    Set JLink Project File to "F:\佳显电子\新程序\电子纸驱动程序更新20191008\AY\6.0\GDE060F3程序示例20190111\project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103VE
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...