#

##

##

    µVision Build Log
    Project:
    E:\STM32F407_demo\stm32f407_demo\project\43\STM32F4_demo_20151203_43\USER\SRAM.uvproj
    Project File Date:  12/01/2015

    Output:
    Build target 'SRAM'
    compiling main.c...
    compiling stm32f4xx_it.c...
    compiling system_stm32f4xx.c...
    compiling epaper.c...
    compiling usart2.c...
    compiling MyLib_w32x16.c...
    compiling MyLib_w32x16aux.c...
    compiling timer.c...
    compiling key.c...
    compiling sdio_sdcard.c...
    compiling usart3.c...
    compiling usartconfig.c...
    compiling delay.c...
    compiling sys.c...
    assembling startup_stm32f40_41xxx.s...
    compiling misc.c...
    compiling stm32f4xx_gpio.c...
    compiling stm32f4xx_fsmc.c...
    compiling stm32f4xx_rcc.c...
    compiling stm32f4xx_syscfg.c...
    compiling stm32f4xx_usart.c...
    compiling stm32f4xx_dma.c...
    compiling stm32f4xx_spi.c...
    compiling stm32f4xx_tim.c...
    compiling stm32f4xx_sdio.c...
    compiling text.c...
    compiling array.c...
    compiling mathchange.c...
    linking...
    Program Size: Code=23812 RO-data=468 RW-data=360304 ZI-data=13752
    FromELF: creating hex file...
    "..\OBJ\SRAM.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\SRAM.AXF"
    Internal DLL Error
    Load "..\\OBJ\\SRAM.AXF"
    Internal DLL Error
    Build target 'SRAM'
    compiling main.c...
    compiling stm32f4xx_it.c...
    compiling system_stm32f4xx.c...
    compiling epaper.c...
    compiling usart2.c...
    compiling MyLib_w32x16.c...
    compiling MyLib_w32x16aux.c...
    compiling timer.c...
    compiling key.c...
    compiling sdio_sdcard.c...
    compiling usart3.c...
    compiling usartconfig.c...
    compiling delay.c...
    compiling sys.c...
    assembling startup_stm32f40_41xxx.s...
    compiling misc.c...
    compiling stm32f4xx_gpio.c...
    compiling stm32f4xx_fsmc.c...
    compiling stm32f4xx_rcc.c...
    compiling stm32f4xx_syscfg.c...
    compiling stm32f4xx_usart.c...
    compiling stm32f4xx_dma.c...
    compiling stm32f4xx_spi.c...
    compiling stm32f4xx_tim.c...
    compiling stm32f4xx_sdio.c...
    compiling text.c...
    compiling array.c...
    compiling mathchange.c...
    linking...
    Program Size: Code=23812 RO-data=468 RW-data=360304 ZI-data=13752
    FromELF: creating hex file...
    "..\OBJ\SRAM.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\SRAM.AXF"
    Internal DLL Error
    Load "..\\OBJ\\SRAM.AXF"
    Internal DLL Error
    Load "..\\OBJ\\SRAM.AXF"
    Internal DLL Error
    Build target 'SRAM'
    compiling main.c...
    compiling stm32f4xx_it.c...
    compiling system_stm32f4xx.c...
    compiling epaper.c...
    compiling usart2.c...
    compiling MyLib_w32x16.c...
    compiling MyLib_w32x16aux.c...
    compiling timer.c...
    compiling key.c...
    compiling sdio_sdcard.c...
    compiling usart3.c...
    compiling usartconfig.c...
    compiling delay.c...
    compiling sys.c...
    assembling startup_stm32f40_41xxx.s...
    compiling misc.c...
    compiling stm32f4xx_gpio.c...
    compiling stm32f4xx_fsmc.c...
    compiling stm32f4xx_rcc.c...
    compiling stm32f4xx_syscfg.c...
    compiling stm32f4xx_usart.c...
    compiling stm32f4xx_dma.c...
    compiling stm32f4xx_spi.c...
    compiling stm32f4xx_tim.c...
    compiling stm32f4xx_sdio.c...
    compiling text.c...
    compiling array.c...
    compiling mathchange.c...
    linking...
    Program Size: Code=23812 RO-data=468 RW-data=360304 ZI-data=13752
    FromELF: creating hex file...
    "..\OBJ\SRAM.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\SRAM.AXF"
    Set JLink Project File to "E:\STM32F407_demo\stm32f407_demo\project\43\STM32F4_demo_20151203_43\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.35b, compiled Sep  2 2011 18:34:46
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 99999993
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots

    Target info:
    ------------
    Device: STM32F407ZE
    VTarget = 3.313V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...