#

##

##

    µVision Build Log
    Project:
    E:\STM32F407_demo\stm32f407_demo\project\quantity_production\STM32F4_demo_20160315_TONGYONG_NEW\USER\SRAM.uvproj
    Project File Date:  01/05/2016

    Output:
    Build target 'SRAM'
    compiling epaper.c...
    linking...
    Program Size: Code=13288 RO-data=468 RW-data=945880 ZI-data=17000
    FromELF: creating hex file...
    "..\OBJ\SRAM.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\SRAM.axf"
    Set JLink Project File to "E:\STM32F407_demo\stm32f407_demo\project\quantity_production\STM32F4_demo_20160315_TONGYONG_NEW\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F407ZE" selected (512 KB flash, 128 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM V8 compiled Nov 28 2014 13:44:46
    Hardware: V8.00
    S/N : 799713843
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F407ZE
    VTarget = 3.325V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.

literal slots * JLink Info: TPIU fitted. * JLink Info: ETM fitted. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: STM32F407ZE VTarget = 3.325V State of Pins: TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 1000 kHz Erase Done. Programming Done. Verify OK.